**APEX-S Valve Controller**

Product Specification

An Elkhart Brass APEX-S Electric Valve Controller shall be provided. The controller shall be no greater than 3.75” wide. The controller shall be rated to IP67 and operate the electric valve from a supply voltage of 12-24 VDC. Controller shall have CAN network capability. Valve position shall be monitored via true position feedback and displayed by 10 LED position indicators. The controller shall include OPEN/CLOSE buttons, a one-touch programmable preset valve position and auto-open/auto-close function. The controller shall include a top-mounted changeable visor available in colors to match the discharge.

**Product Features**

* Valve control with 10 segment LEDs for position indication
* CAN network compatible
* Oversized buttons for easy gloved-hand operation
* Programmable preset for automatic valve positioning
* AUTO open/close feature for quick operation
* Visors in NFPA colors to match pump discharge colors