**EXM2 HANDHELD REMOTE CONTROLLER PACKAGE (7015X2) DS and GW)**

**Product Specification**

Wireless Controller and vehicle mounted RF/CAN Gateway shall have an IP67 and NEMA 4 rating with reverse polarity and circuit board moisture protection; shall provide user interface for wireless remote control for monitor up/down, left/right rotation, stow, deploy, horizontal and vertical automatic oscillation, nozzle control functions, and valve control functions; shall provide the user feedback for power on, valve open position, valve closed position, and valve preset position; shall provide programming capability for horizontal center position, horizontal stops, stow and deploy positions, block-out zones, and motor speeds fast or slow; shall be radio frequency compatible; shall allow for electrical control and feedback at a distance of up to 400 meters; wireless controller shall have a rechargeable lithium-ion battery pack that allows for up to 24 hours of continuous use between charges; shall include a IP67 and NEMA 4 rated charging/docking station compatible with both 12VDC and 24VDC power supply; charging of wireless remote shall be via induction charging technology.