**EXM2 JOYSTICK CONTROLLER (7030X2)**

**Product Specification**

Panel Mount Joystick with NEMA 4 rating shall include integrated CAN output and connect directly to monitor without the need for an intermediate communication module; shall provide user interface for proportional monitor up/down, left/right rotation, stow, deploy, programmable horizontal and vertical automatic oscillation, nozzle control functions, and valve control functions; shall provide the user feedback for power on, valve open position, valve closed position, and valve preset position; shall provide programming capability for horizontal and vertical stops, stow and deploy positions, block-out zones, and motor speeds fast or slow.