**EXM2 PANEL MOUNT CONTROLLER (7010X2)**

**Product Specification**

Controller shall have an IP67 and NEMA 4 rating with reverse polarity and circuit board moisture protection; control circuitry shall use programmable integrated circuit technology for monitor up/down, left/right rotation, stow, deploy, horizontal and vertical automatic oscillation, nozzle control functions, and, valve control functions; shall provide the user feedback for power on, valve open position, valve closed position, and valve preset position; shall provide programming capability for horizontal center position, horizontal stops, stow and deploy positions, block-out zones, and motor speeds fast or slow; shall be CAN network compatible; shall be compatible with both 12VDC and 24VDC power supply.