**EXM2 POSITION DISPLAY MODULE (7051X2)**

**Product Specification**

Position Feedback Display shall provide user feedback for horizontal and vertical monitor positioning based on absolute position sensors, shall indicate when monitor has reached programmed stow position, shall provide available range of motion through back-light feature; shall be CAN compatible; shall be compatible with both 12VDC and 24VDC.